규 격 시 방 서
품목	비디오프로젝터	품명	EB-685W
용도	영사용 기기	밝기	3,500lm ANSI
A. 제품 사진 안내 3LCD VIDEO PROJECTOR

규 격 시 방 서
품목	비디오프로젝터	품명	EB-685W
용도	영사용 기기	밝기	3,500lm ANSI
B. 제품 특징 안내
초단초점 비디오프로젝터 EB-685W
□ 참여도 높은 학습경험을 제공하는 3LCD 프로젝터
3LCD 기술을 통한 선명한 이미지 구현 및 레인보우 현상 없는 선명한 화면
밝기 3,500lm 통한 생생한 색상으로 강의의 질 향상
□ 눈의 피로 최소화
최대 100인치 화면을 통한 강의실 모든 학생들이 콘텐츠 학습 가능
어느 각도에서도 눈부심 없이 선명한 이미지 제공 및 눈의 피로 최소화
□ 교육환경 최적화
교실 또는 강의실에서 많은 사람에게 화면 설명하기 용이
□ 기타 기능 지원
세팅 플레이트를 통한 3축 조절 기능으로 투사 이미지를 원하는 위치에 고정
ECO모드 사용 시, 램프 교체 없이 최대 10,000시간 사용
향상된 방진 성능의 에어 필터 장착 가능

규 격 시 방 서
품목	비디오프로젝터		품명	EB-685W
용도	영사용 기기		밝기	3,500lm ANSI
C. 제품 규격 안내
투사방식			천정 마운트 전면 / 천정 마운트 후면 데스크탑 전면 / 데스크탑 후면 테이블 프로젝션 전면 / 테이블 프로젝션 후면
부분별 사양	LCD	크기	0.59-inch (D9, C2 Fine)
		해상도	WXGA (1280 x 800 픽셀)
	렌즈	화면비율	16:10
		초점 거리	3.7 mm
	광원	방식	Lamp (250 W UHE)
		수명	5000 시간 (Normal)
화면 크기			60" ~ 100" [35.4 - 60.1cm]
			74.3" screen 44.3cm
			투사율 0.28 (Zoom: Wide) 0.37 (Zoom: Tele)
밝기			3,500 lm
명암비			14,000:1
크기	최대 (W x H x D)		367 x 187 x 400 mm
	다리 제외 (W x H x D)		367 x 149 x 400 mm
무게 (케이블 커버 제외)			약 5.7Kg
전기 사양	필요 전원 공급		AC 100 - 240V, 50/60 Hz, 3.8 - 1.7A
	정격 소비 전력		354W (Normal) / 309W (Eco)
키스톤 보정			지원
팬소음			38dB (Normal), 30dB (ECO)
화면 분할 (Split Screen)			지원
엣지 브랜딩			지원 안함
퀵 코너 조정			지원
Video I/O	입력	아날로그	RGB, 컴포넌트, RGB-Video : D-sub 15pin – 2 (Blue molding, Black molding) *Computer 2: In common with Monitor out, RCA - 1 (Yellow)
		디지털	HDMI(CEC) : 3* *HDMI 1: In common with MHL
	출력	아날로그	RGB, RGB-Video : D-sub 15pin - 1 (Black molding)
		디지털
USB I/O	Type A		1 (USB Display, Mouse, K/B, Control, Firmware update, Copy OSD Settings)
	Type B		1 (USB Display, Mouse, K/B, Control, Firmware update, Copy OSD Settings
Audio I/O	입력		Stereo mini : 3
	출력		Stereo mini : 1
네트워크	유선		RJ45 : 1(100Mbps)
	무선		Type A (ELPAP10 : Option) : 1